Augusta Centennial Hall – Hirers Information 2026
SIMPLY SWITCH ON THE POWERPOINT LABELLED “AUDIO” ON THE WALL BEHIND THE 
SERVER RACK – ALL AMPLIFIERS AND THE MIXER WILL POWER UP
  A. Setup – Bluetooth or direct stereo cable to  wall box – DEFAULT SETTING 
Simply connect to the bluetooth device WP225 or use a 3.5ml stereo cable from your device and raise the volume on your device accordingly. Inputs 9/10 are the relevant mixer channels.
  B. Setup – Laptop presentation with radio mics                                                                           The Centennial Hall Committee will assign someone to setup the built in mixer to facilitate the use of wireless mics and the data projector. A long HDMI cable is fixed to the server rack and cannot be extended beyond its available length. Audio is on channels 11/12 on the mixer.
Should the above setup also require desktop mics for a panel situation, 4 mics can be deployed on desk stands and connected to the mixer on channels 1-4.
  C . Volume levels                                                                                                                     Master levels have been set for the output of the mixer to the amplifiers, with the 2 faders marked SUB and FOH on the far right of the mixer set at optimum positions for a correct balance. These will already be ONt. It is recommended you do not adjust these faders from the set position. Simply choose your input device, as per the labels on the fader, press the ON button for that source and raise that source fader to the desired level.
  D. Setup – Hirers with external mixers 
The PA system is designed to manage direct access to the following 3 amplifier inputs via the small stagebox/snake located at the bottom of the rack:
· FOH satellites speakers mounted on the wall
· 2 x stage monitors as Aux 1 and Aux 2 on the left and right of the stage  Single subwoofer on floor below stage
	The default mode is FOH speakers are currently connected to the Yamaha mixer’s Main output via the Stagebox inputs 1 and 2.
The SUB is currently connected to the Yamaha mixer’s SUB output via stagebox input 5.
Aux inputs 3 and 4 from the stage box are currently connected to the stage monitor amps inputs 1 / 2 which feed the left and right stage monitors – the inputs are ready for a hirer’s AUX connections.
YOU MUST RETURN THE CONNECTIONS TO THIS DEFAULT. FAILURE TO DO SO WILL 
RESULT IN NO FURTHER BOOKINGS BEING PERMITTED
PLEASE NOTE: The stagebox inputs have a tang to prevent accidental disconnection. The tang is located above the XLR input. Please disconnect carefully.
Please connect your external mixer as per the labels on the stagebox. Note input 6 is not in use. The 3 amplifiers in use have the following locked settings:   


	
	· FOH channels 	– HPF [lowcut] of 105hz (inputs 1 and 2)
· Sub 	– LPF [high cut] of 110hz (input 5)
· Aux channels	– No EQ settings (inputs 3 and 4)



